A close up of a map

Description automatically generated

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | logo | | | |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
| **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** | | | | | | | | | |
| 1813 McCullough Blvd. 38801 ~ Post Office Box 1427 38802 ~ Tupelo, MS 38801 ~ Ph 1-800-737-8272 ~ Fax 662-844-8511 | | | | | | | | | |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **SECURITY SCREEN SPECIFICATIONS** | | | | | | | | |
|  | **#125 ECONOMY SERIES** | | | | | | | | |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **A. Sub-Frame: Extruded aluminum 6063-T5, .062 wall thickness,** | | | | | | | |  |
|  | **1.437" x 1.065 single hollow. Weight per ft .360** | | | | | |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **B. Main Frame: Extruded aluminum 6063-T5, 1.390" Wide x .966" Height,** | | | | | | | | |
|  | **.060 wall thickness. Weight per ft .340** | | | | |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **C. Corner Gussets: Shall be .250 solid aluminum or welded corners.** | | | | | | | |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **D. Spreader Bar: Extruded aluminum 6063-T5, 1.00" x .400" with .060 wall** | | | | | | | | |
|  | **thickness.** | |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **E. Wire Mesh: Stainless steel with natural or painted finish or perforated** | | | | | | | | |
|  | **with powder coat paint, .028 or .035 12 x 12 mesh.** | | | | | |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **F. Anchor Bar: Extruded aluminum 6063-T5, 1.00" wide x .060 wall thickness.** | | | | | | | | |
|  | **Screws not to exceed 4" apart.** | | | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **G. Hinge: Top or side pivot - 1/4" x 2-3/8" SST pivot rod.** | | | | | | |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **H. Latches: Stainless steel barrel bolt latches or optional single point** | | | | | | | |  |
|  | **release latch.** | |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  | **I. Finish: Mill Finish, Bronze, White** | | | |  |  |  |  |  |